- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### End Suction Pump

Flow up to | 750 m3/hr
Head up to | 170 m
Temperature up to | 120°C
DN | 32-150
Design Features | End Suction Top Discharge Mounting: Horizontal Stage: Single Back Pullout design Closed Impeller Mechanical Seal/ Gland Packing Grease lubricated antifriction bearings
Optional Features | Mounting: Centreline/ Vertical Semi-open Impeller Oil lubricated antifriction bearings
Material of Construction | Cast Iron, Bronze, Ductile Iron, Cast Steel, Nil Resist, Stainless Steel, Duplex Stainless Steel & Special alloys
Applications | General Industry Chemical & Process Water Supply Building Service Firefighting Intigation Sprinkler system
Prime movers | Electric motors Diesel Engines

### FAQs of End Suction Pump

An End Suction Pump is a single-stage centrifugal pump designed for reliable liquid transfer in industrial, commercial, and utility applications.

The pump can deliver flow rates up to 750 m³/hr.

The pump delivers a head up to 170 meters.

The pump is suitable for liquid temperatures up to 120°C.

The pump is available in sizes ranging from DN 32 to DN 150.

Enquiry Now