- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Floating Ball Valve 2 Pcs Design Soft & Metal Seated

### Model No: U-Series

Model: | U-Series
Size Range: | 15 NB to 150 NB
Pressure Rating: | ASME Class #150 to Class #2500
Design Standard: | ISO 17292, API 608, API 6D
Testing Std: | API 6D / BS EN ISO 5208 / API 598 / BS EN 12266-1
Face to Face: | ASME B 16.10
End Connection: | Flanged
Seat Design: | PTFE / MPTFE / TFM 1600 / RPTFE / DEVLON / PEEK/CRYO PEEK / PCTFE / METAL (CRC /TCC /ST)

### FAQs of Floating Ball Valve 2 Pcs Design Soft & Metal Seated

A Floating Ball Valve is a quarter-turn valve designed for reliable shutoff and flow isolation. This model is available with both soft seats and metal seats, making it suitable for a wide range of pressure, temperature, and industrial service conditions.

The valve is available in sizes ranging from 15 NB to 150 NB.

Yes. The metal seated configuration is specially designed for high temperature and severe service conditions.

The valve complies with:

- ASME B16.10
Enquiry Now