- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Dual Plate Check Valves

### Model No: IVDPCV

Model: | IVDPCV
Size Range: | 25NB to 1500NB
Pressure Rating: | ASME Class #150, #300, #600
Design Standard: | API 594
Testing Std: | API 598
Face to Face: | API 594
End Connection: | Flanged / Wafer
Seat Options: | EPDM / PTFE / 13 Cr. / SS316 / SS304 / ST.

### FAQs of Dual Plate Check Valves

A Dual Plate Check Valve is a compact non-return valve designed to prevent reverse flow in piping systems. It uses two spring-loaded plates that open with forward flow and close automatically when flow stops or reverses.

The valve is available in sizes ranging from 25 NB to 1500 NB

Yes. The spring-assisted dual plate design provides quick closing action, which helps minimize water hammer effects in piping systems.

The valve complies with:

- API 594

Enquiry Now