- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Rubber Encapsulated Disc Butterfly Valve

### Model No: IVGE / IVTLE

Model: | IVGE / IVTLE
Size Range: | 50 NB to 350 NB
Pressure Rating: | Upto PN10
Design Standard: | API 609 , EN593, IS 13095
Testing Std: | API 598 / ANSI-FCI 70-2 / EN 12266-1
Face to Face: | API 609 Cat-A /ISO 5752 Tab 5/ BS EN558
End Connection: | Wafer / Lugged
Seat Design: | Bonded

### FAQs of Rubber Encapsulated Disc Butterfly Valve

A Rubber Encapsulated Disc Butterfly Valve is a resilient seated butterfly valve where the disc is fully coated or encapsulated with rubber for enhanced sealing, corrosion resistance, and smooth operation.

These valves are available in sizes ranging from 50 NB to 350 NB.

The valve is designed for pressure ratings up to PN10..

In bonded seat design, the resilient seat is permanently bonded to the valve body, improving sealing reliability and reducing the chances of seat displacement.

Enquiry Now