- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### ECO PP HORIZONTAL PUMPS

### Economy Series

Economy Series include Compact Centrifugal Pumps in Polypropylene construction, extensively used for the circulation of various chemicals having an externally mounted seal (Teflon bellow) arrangement.

#### Duty Conditions :

Capacity (Q): | up to 28 m3/hr
Head (H): | up to 28m
Opt. Temperature: | 0°C to 75°C
Motor Rating | up to 2.2 kW

### Jumbo Series :

Jumbo Series include Compact Centrifugal Pumps in Polypropylene construction, extensively used for the circulation of various chemicals having an externally mounted seal (Teflon bellow) arrangement.

#### Duty Conditions :

Capacity (Q): | up to 200 m3/hr
Head (H): | up to 65m
Opt. Temperature: | 0°C to 75°C
Motor Rating | up to 30 kW

### Standard Series :

Standard Series include Compact Centrifugal Pumps in Polypropylene construction, extensively used for the circulation of various chemicals having an externally mounted seal (Teflon bellow) arrangement.

#### Duty Conditions :

Capacity (Q): | up to 50 m3/hr
Head (H): | up to 50m
Opt. Temperature: | 0°C to 75°C
Motor Rating | up to 15 kW

### FAQs of Eco PP Horizontal Pumps

All three series—Economy, Jumbo, and Standard—are constructed from Polypropylene, making them highly resistant to corrosive chemicals and suitable for chemical circulation applications.

Each pump series uses an externally mounted Teflon bellow mechanical seal, ensuring excellent leakage resistance and reliable operation even with aggressive chemicals.

- Economy Series: For small to medium applications (up to 28 m³/hr, 28m head).
- Standard Series: Medium-duty applications (up to 50 m³/hr, 50m head).
- Jumbo Series: Heavy-duty, high-flow applications (up to 200 m³/hr, 65m head).

Each series is designed to meet different flow and head requirements based on industrial needs.

All pump series operate efficiently between 0°C and 75°C, making them suitable for a wide range of chemical process temperatures.

These pumps are used in chemical processing, acid/alkali transfer, scrubber circulation, electroplating, water treatment, and general industrial applications requiring corrosion-resistant fluid handling.

Enquiry Now