- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Standard Horizontal Split Case Pump

Flow up to | 3400 m³/hr
Head up to | 235m
Temperature up to | 120°C
DN | 50 - 400
Design Features | Mounting inline Horizontal stage: Single/Double Suction Impellers Shaft with Sleeves Grease lubricated antifriction bearing Mechanical seal/ Gland Packing
Optional Features | Mounting Vertical
Material of Construction | Casing - Cast Iron Impeller- Cast Iron/ Bronz / SS (CF8M)
Applications | Water Supply General Industry Building Service Fire Fighting Spray Imigation District heating
Prime movers | Electric motors

### FAQs of Standard Horizontal Split Case Pump

A Standard Horizontal Split Case Pump is a high-capacity centrifugal pump designed for efficient water transfer and circulation in industrial, commercial, and municipal applications.

This pump can handle flow rates up to 3400 m³/hr.

The pump delivers a head up to 235 meters.

It is designed to handle liquids with temperatures up to 120°C.

The pump is available with Single Suction or Double Suction Impellers depending on the application requirement.

Enquiry Now