- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Bonded Seat Butterfly Valve

### Model No: IVGKB/IVTLB/IVDF

Model: | IVGKB/IVTLB/IVDF
Size Range: | 40 NB to 1200 NB
Pressure Rating: | Upto ASME Class #150
Design Standard: | API 609 , EN593, IS 13095
Testing Std: | API 598 / ANSI-FCI 70-2 / EN 12266-1
Face to Face: | API 609 Cat-A /ISO 5752 Tab 5/ BS EN558
End Connection: | Wafer / Lugged / Double Flanged
Seat Design: | Bonded

### FAQs of Bonded Seat Butterfly Valve

A Bonded Seat Butterfly Valve is a quarter-turn valve designed for reliable flow control and shut-off applications. The resilient seat is permanently bonded to the valve body, ensuring leak-tight sealing and improved durability.

These valves are available in sizes ranging from 40 NB to 1200 NB, making them suitable for both small and large pipeline systems.

The valve is designed for pressure ratings up to ASME Class #150.

No. The bonded seat design minimizes wear and reduces maintenance requirements, ensuring long-term reliable operation.

Enquiry Now