- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Dry Claw Vacuum Pumps

100% Dry Pumping (No Sealing Fluid)
Current Range includes 5 models, from 60 m3/hr to 600 m3/hr
Continuous Vacuum: Up to 100 mbar(A)
Built-In Air Cooling
Optional VFD for Greater Control
Minimal Maintenance
Versatile Applications

### FAQs of Dry Claw Vacuum Pumps

A Dry Claw Vacuum Pump is a positive displacement vacuum pump that uses claw-shaped, non-contacting rotors to generate vacuum without oil or sealing fluid in the compression chamber.

The Dry Claw Vacuum Pump range includes 5 models, with capacities from 60 m³/hr to 600 m³/hr.

These pumps can achieve a continuous vacuum of up to 100 mbar(A).

Dry pumping ensures the compression chamber operates without oil, water, or sealing fluids, providing contamination-free vacuum generation.

Enquiry Now