- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Horizontal Monobloc Pump

Flow up to | 34 m³/hr
Head up to | 95 m
Temperature up to | 110°C
DN | 25-32
Design Features | Mounting: Horizontal Stages: 2 to 7 Corrosion proof wetted components Mechanical Seal with EPDM/Viton clastomers
Optional Features | Self priming models Electronic control motor Single & Three phase
Material of Construction | Casing-SS (304/316L)/Cast Iron Impeller-S5 (304/316L)
Applications | Water Supply Pressure Boosting Industrial Washing Sprinkling Systems General Industry
Prime movers | Electric motors

### FAQs of Horizontal Monobloc Pump

The pump offers a flow capacity of up to 34 m³/hr and supports multiple head configurations depending on the number of stages, suitable for a wide range of industrial and utility applications.

The pump is designed to operate safely with liquids up to 110°C, making it ideal for hot water, industrial processes, and high-temperature cleaning systems.

Key design characteristics include:

- Horizontal mounting
- 2 to 7 stages for higher pressure requirements
- Corrosion-proof wetted components
- Mechanical seal with EPDM or Viton elastomers for durability and chemical resistance

Yes. Optional configurations include:

- Self-priming models
- Electronic control motors
- Single-phase or three-phase motor options

The pump operates using electric motors, available in both single-phase and three-phase variants depending on the requirement.

Enquiry Now