- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Vertical Sump Pump

Flow up to | 750 m3/hr
Head up to | 220 m
Temperature up to | 150°C
DN | 32-200
Design Features | Vertical wet pit volute pump with dry motor Stage: Single Closed Impeller Oil lubricated bearing arrangement Antifriction bearing Mechanical Seal/ Gland Packing
Optional Features | Semi – open Impeller
Material of Construction | Cast Iron, Bronze, Ductile Iron, Cast Steel, Nil Resist, Stainless Steel, Duplex Stainless Steel & Special alloys
Applications | Emergency oil pump Dewatering
Prime movers | Electric motors

### FAQs of Vertical Sump Pump

A Vertical Sump Pump is a vertical wet pit centrifugal pump designed for handling liquids collected in pits, tanks, and underground sumps while keeping the motor safely above the liquid level.

The pump can handle flow rates up to 750 m³/hr.

The pump delivers a head up to 220 meters.

The pump is suitable for liquid temperatures up to 150°C.

The pump is available in sizes ranging from DN 32 to DN 200.

Enquiry Now