- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Multistage Ring Section Pump

Flow up to | 1000 m3/hr
Head up to | 1800 m
Temperature up to | 160°C
DN | 32-250
Design Features | Mounting: Horizontal Stage: 3 to 15 Radial Flow Impellers with vane diffusers Mechanical Seal/Gland Packing Grease lubricated antifriction Bearings
Optional Features | Mounting: Centreline/Vertical Multi-Outlet design for axial thrust Bush Bearing/Roller Bearing
Material of Construction | Cast Iron, Bronze, Ductile Iron, Cast Steel, Nil Resist, Stainless Steel, Duplex Stainless Steel & special alloys
Applications | Mine dewatering Descaling in Steel mills Boiler Feed application Reverse Osmosis for Desalination Plants water Supply General Industry Fire fighting
Prime movers | Electric motors Diesel Engine Steam Turbine

### FAQs of Multistage Ring Section Pump

A Multistage Ring Section Pump is a high-pressure centrifugal pump designed with multiple impellers to achieve very high heads for demanding industrial applications.

The pump can deliver flow rates up to 1000 m³/hr.

The pump delivers a head up to 1800 meters.

The pump is suitable for liquid temperatures up to 160°C.

The pump is available in sizes ranging from DN 32 to DN 250.

Enquiry Now