- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Dry Screw Vacuum Pumps

100% Dry Pumping (No Sealing Fluid)
6 models from 60 m3/hr to 1500 m3/hr
Manufacturing capability of 1000 m/c per annum
Hybrid Variable Pitch Design, high volumetric efficiency
Internals available as per process requirements and applications

### FAQs of Dry Screw Vacuum Pumps

A Dry Screw Vacuum Pump is a high-performance vacuum pump that uses two non-contacting screw rotors to create vacuum without the use of sealing fluids or lubricants in the compression chamber.

Dry Screw Vacuum Pumps are available in capacities ranging from 60 m³/hr to 1,500 m³/hr.

It means the pumping chamber operates completely free of oil, water, or any sealing fluid, ensuring clean, contamination-free vacuum generation.

The hybrid variable pitch screw design optimizes gas compression across the rotor length, delivering higher efficiency, improved pumping speed, and better energy savings.

Enquiry Now