- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Cast Steel – Gate, Globe & Swing Check Valves

### Model No: IVGTC / IVGLF / IVSCC

Model: | IVGTC / IVGLF / IVSCC
Size Range: | 50NB to 1000NB
Pressure Rating: | ASME Class #150, #300, #600
Design Standard: | API 600 / BS 1873 / BS 1868
Testing Std: | API 598
Face to Face: | ASME B16.10
End Connection: | Flanged & Butt Weld
Trim Options: | 1 / 5 / 8 / 12/ 16

### FAQs of Cast Steel – Gate, Globe & Swing Check Valves

These are industrial cast steel valves designed for flow isolation, regulation, and non-return applications in high pressure and high temperature piping systems.

- Gate Valve – Used for full open or full close isolation service
- Globe Valve – Used for flow regulation and throttling
- Swing Check Valve – Prevents reverse flow automatically

The valves are available in sizes ranging from 50 NB to 1000 NB.

Yes. Cast steel construction and suitable trim selections make these valves ideal for high temperature and high pressure services.

A Swing Check Valve automatically prevents reverse flow in the pipeline, protecting pumps, compressors, and process equipment.

Enquiry Now