- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Drypit Nonclog Sewage/ Wastewater Pump

Flow up to | 8000 m3/hr
Head up to | 70 m
Temperature up to | 90°C
DN | 50-800
Design Features | End Suction Top Discharge Mounting: Horizontal Stage: Single Casing with hand hole inspection cover Mechanical seal/ Gland Packing Large Free Passage up to 200 mm
Optional Features | Cast Iron, Bronze, Ductile Iron, Cast Steel, Nil Resist, Stainless Steel, Duplex Stainless Steel & special alloys
Material of Construction | Cast Iron, Bronze, Ductile Iron, Cast Steel, Nil Resist, Stainless Steel, Duplex Stainless Steel & Special alloys
Applications | Municipal Raw Sewage transfer Sewage treatment plants Effiument treatment plants Dirty water in industry Sugar Mills
Prime movers | Electric motors

### FAQs of Drypit Nonclog Sewage/ Wastewater Pump

A Drypit Nonclog Sewage / Wastewater Pump is a heavy-duty centrifugal pump designed for handling sewage, wastewater, and liquids containing solids without clogging.

The pump can handle flow rates up to 8000 m³/hr.

The pump delivers a head up to 70 meters.

The pump is suitable for liquid temperatures up to 90°C.

The pump is available in sizes ranging from DN 50 to DN 800.

Enquiry Now