- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Floating Ball Valve 3 Pcs Design Soft Seated

### Model No: Standard Series

Model: | Standard Series
Size Range: | 15 NB to 50 NB
Pressure Rating: | ASME Class #800
Design Standard: | ISO 17292, API 608
Testing Std: | BS EN ISO 5208 / API 598 / BS EN 12266-1
Face to Face: | Manufacturing Standard
End Connection: | Socket Weld, Screwed & Butt Weld
Seat Design: | PTFE / MPTFE / TFM 1600 / RPTFE / DEVLON / PEEK

### FAQs of Floating Ball Valve 3 Pcs Design Soft Seated

A Floating Ball Valve with 3-piece design is a compact quarter-turn valve consisting of three body sections. This design allows easy dismantling and maintenance without removing the valve from the pipeline.

The valve is available in sizes ranging from 15 NB to 50 NB.

These valves are primarily designed for isolation applications. Continuous throttling is generally not recommended.

The valve is designed for:

- ASME Class #800
Enquiry Now