- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Vertical Turbine Pump

Flow up to | 40000 m3/hr
Head up to | 450 m
Temperature up to | 80°C
DN | 100-2000
Design Features | Vertical wet pit Stage Single/ Multistage Closed Impeller Above or Below floor discharge Pumped medium lubricated line shaft bearings Non pull out bowl/rotating element antifriction bearings
Material of Construction | Cast Iron, Bronze, Ductile Iron, Mild Steel, Cast Steel, Nil Resist, Stainless Steel, Duplex Stainless Steel & Special alloys
Applications | Water Supply Irrigation Cooling water for Power Plant flood Control Condensate Extraction General Industry Fire fighting
Prime movers | Electric motors Diesel Engines via right angle gear box Stem Turbine via right angle gear box

### FAQs of Vertical Turbine Pump

A Vertical Turbine Pump is a high-capacity vertical centrifugal pump designed for pumping water and other liquids from deep wells, wet pits, reservoirs, and large water sources.

The pump can deliver flow rates up to 40,000 m³/hr.

The pump delivers a head up to 450 meters.

The pump is suitable for liquids with temperatures up to 80°C.

The pump is available in sizes ranging from DN 100 to DN 2000.

Enquiry Now