- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Tri Lobe Blowers

Oil-free air with contactless sealing, maintenance-free
High Efficiency
Different configurations available for special applications
16 m3/hr to 9,000 m3/hr in single stage up to 1bar(A)

### FAQs of Tri Lobe Blowers

A Tri Lobe Blower is a positive displacement blower featuring three precision-engineered lobes that deliver smooth, pulsation-free, and oil-free airflow for a wide range of industrial applications.

Tri Lobe Blowers are available in capacities ranging from 16 m³/hr to 9,000 m³/hr in a single-stage configuration.

These blowers can operate up to 1 bar(A) in single-stage applications.

Contactless sealing eliminates internal friction between rotating components, reducing wear, increasing efficiency, and significantly extending blower life.

Enquiry Now