- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Centrifugal Blowers

Flow Rates:Up to 6,000m3/hr
Range:Max. Pressure 260 mbar and Max. Vacuum 180 mbar
Technology:100% Oil free & Gearlesstechnology
Customizable according to ambient temperature efficiency class
Virtually maintenance – free
Available in seven different configurations based on impeller type
Heavy duty & continuous operations

### FAQs of Centrifugal Blowers

A Centrifugal Blower is a high-performance air-moving device that uses centrifugal force to deliver large volumes of air at low to medium pressure for industrial applications.

Centrifugal Blowers can deliver air flow rates of up to 6,000 m³/hr.

- Maximum Pressure: 260 mbar
- Maximum Vacuum: 180 mbar

Yes, our Centrifugal Blowers are designed with 100% oil-free operation, ensuring clean and reliable airflow for your industrial applications.

Enquiry Now