- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Side Channel Blowers

Flow Rates: Up to 2,500 m3/hr
Range: Max. Pressure 1040 mbar and Max. Vacuum 740 mbar
Configurations: Available in Single/Three Phase & Single/Double/Triple Stage Configurations
Technology: 100% Oil free & Gearless technology
ADC-12 MOC offering compact, lightweight & durable assembly

### FAQs of Side Channel Blowers

A Side Channel Blower is a non-contact, dynamic air blower designed to deliver high-pressure and vacuum performance with completely oil-free operation. It is ideal for industrial applications requiring clean, reliable airflow.

Side Channel Blowers can deliver air flow rates of up to 2,500 m³/hr.

- Maximum Pressure: 1040 mbar
- Maximum Vacuum: 740 mbar

Gearless operation reduces mechanical wear, minimizes maintenance, lowers noise levels, and ensures longer service life.

Enquiry Now