- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### PTFE Seated Butterfly Valve

### Model No: IVTFE

Model: | IVTFE
Size Range: | 50 NB to 350 NB
Pressure Rating: | Upto PN10
Design Standard: | EN593, IS 13095
Testing Std: | API 598 / ANSI-FCI 70-2 / EN 12266-1
Face to Face: | ISO 5752 Tab 5/ BS EN558
End Connection: | Wafer
Seat Design: | Replaceable [PTFE / GFT with Backup Ring]

### FAQs of PTFE Seated Butterfly Valve

A PTFE Seated Butterfly Valve is a high-performance butterfly valve designed with a PTFE or GFT replaceable seat for handling corrosive chemicals, aggressive media, and high-purity applications.

The valve is available in sizes ranging from 50 NB to 350 NB.

The valve is designed for pressure ratings up to PN10..

GFT (Glass Filled PTFE) is a reinforced PTFE material that offers improved strength, wear resistance, and dimensional stability for demanding applications.

Enquiry Now