- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Single Piece Wafer Type Check Valves

### Model No: IVC / IVCT

Model: | IVC / IVCT
Size Range: | 25NB to 900NB
Pressure Rating: | Upto PN16
Design Standard: | IV Standard
Testing Std: | API 598
Face to Face: | Manufacturing Standard
End Connection: | Wafer
Seat Options: | Replaceable

### FAQs of Single Piece Wafer Type Check Valves

A Single Piece Wafer Type Check Valve is a compact non-return valve designed to prevent reverse flow in pipelines. Its lightweight wafer-type construction allows easy installation between flanges while ensuring reliable flow control.

The valve is available in sizes ranging from 25 NB to 900 NB.

A replaceable seat design allows the sealing seat to be changed or replaced during maintenance, helping extend valve life and reduce maintenance costs.

Yes. The replaceable seat arrangement allows easier servicing and reduces the need for complete valve replacement.

Enquiry Now