- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Liquid Ring Vacuum Pumps

### Model No: 2BE3 / P2620

- Large liquidring vacuumpumps with superior corrosion resistance
- Topdischarge whicheliminatesneedfortrench Self-recirculatingsealwater,reducingneedforexternalseal watersource
- Capacityof4,000to23,000CFMwithvacuumto29+”HgV

### FAQs of End of Line Robuschi

The pump is built with superior corrosion-resistant materials, making it suitable for handling moist, corrosive, or abrasive gases commonly found in industrial vacuum applications.

The top-discharge outlet eliminates the need for trenches or floor modifications. It also helps in easier installation, simplifies piping layout, and improves overall operational efficiency.

No. The pump features a self-recirculating seal-water system, significantly reducing or eliminating the requirement for an external seal-water supply. This lowers water consumption and operating costs.

The 2BE3 / P2620 offers a wide performance range with capacities from 4,000 to 23,000 CFM, making it suitable for medium to heavy-duty industrial vacuum applications.

This model can achieve vacuum levels of up to 29+ inches of HgV, making it ideal for applications requiring deep and stable vacuum performance.

Enquiry Now