- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Soft Seated Double Offset Butterfly Valve

### Model No: IVEX-T

Model: | IVEX-T
Size Range: | 50 NB to 600 NB
Pressure Rating: | ASME Class #150, #300
Design Standard: | API 609 , EN593
Testing Std: | API 598 / ANSI-FCI 70-2 / EN 12266-1
Face to Face: | API 609 Cat-B
End Connection: | Wafer / Lugged / Double Flanged
Seat Design: | Replaceable [PTFE / GFT]

### FAQs of Soft Seated Double Offset Butterfly Valve

A Soft Seated Double Offset Butterfly Valve is a high-performance butterfly valve designed with a double offset disc arrangement and soft replaceable seat for improved sealing, reduced wear, and smooth operation in demanding industrial applications.

The valve is available in sizes ranging from 50 NB to 600 NB.

Yes. The valve is suitable for both isolation and throttling services with precise flow control.

The valve is designed for:

- ASME Class #150
- ASME Class #300

Enquiry Now