- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Multi Pump Booster

Flow up to | 900 m3/hr
Head up to | 235 m
Temperature up to | 120°C
DN | 32-100
Design Features | Multi-pump Pressure Boosting system from two up to eight pumps in Stainless Steel construction, Fitted on a common baseplate with vibration dampers
Optional Features | Horizontal / Vertical Pumps Variety of Panels with floating VFD/ with dedicated VFD/ without VFD, with PLC/without PLC, panels with customized requirements.
Material of Construction | Casing – SS (304/316L) Cast Iron Impeller – SS (304/316L)
Applications | Pressure Boosting for Commercial complexes, Hotels, Industries, etc.
Prime movers | Electric motors

### FAQs of Multi Pump Booster

A Multi Pump Booster System is an automatic pressure boosting solution that uses multiple pumps operating together to maintain constant water pressure in commercial and industrial applications.

The pump can handle flow rates up to 900 m³/hr.

The pump delivers a head up to 235 meters.

The pump is suitable for liquid temperatures up to 120°C.

The pump is available in sizes ranging from DN 32 to DN 100.

Enquiry Now