- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Engineered Vacuum Systems

100% Dry Pumping
Combination of Dry Screw Vacuum Pumps and Mechanical Vacuum Boosters
Standardized products for Chemical & Pharma, API manufacturing.
Short lead time of 7-10 days (Typically) because of standardization.
Current Range varies from 800 m3/hr to 30,000 m3/hr

### FAQs of Engineered Vacuum Systems

An Engineered Vacuum System is a customized industrial vacuum solution designed for continuous and efficient vacuum generation in chemical, pharmaceutical, and API manufacturing processes.

The system uses a combination of Dry Screw Vacuum Pumps and Mechanical Vacuum Boosters for reliable and 100% dry vacuum operation.

100% dry pumping means the system operates without oil or liquid contact inside the pumping chamber, reducing contamination and maintenance requirements.

Because dry systems prevent oil contamination, maintain process purity, and comply with strict industrial hygiene and production standards.

Enquiry Now