- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Triple Offset High Performance Butterfly Valve

### Model No: IVEX

Model: | IVEX
Size Range: | 80 NB to 750 NB
Pressure Rating: | ASME Class #150, #300, #600
Design Standard: | API 609 , EN 593
Testing Std: | API 598 / ANSI-FCI 70-2 / EN 12266-1
Face to Face: | API 609 Cat-B
End Connection: | Wafer / Lugged / Double Flanged
Seat Design: | Laminar Seal

### FAQs of Triple Offset High Performance Butterfly Valve

A Triple Offset High Performance Butterfly Valve is a premium industrial butterfly valve designed with three offsets to eliminate friction between the disc and seat during operation. It provides tight shutoff, high durability, and excellent performance in high-pressure and high-temperature applications.

The valve is available in sizes ranging from 80 NB to 750 NB.

A laminar seal consists of layered metallic sealing elements designed to provide flexible, tight sealing under demanding operating conditions.

Yes. The valve can be used for both isolation and throttling applications with precise flow control.

Enquiry Now