- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Vertical Inline Pump

Flow up to | 155 m3/hr
Head up to | 235 m
Temperature up to | 120°C
DN | 25-100
Design Features | Mounting: Vertical Inline Stage: 2 to 24 Antifriction Bearings Corrosion proof wetted components Mechanical Seal with EPDM/ Viton elastomers Connection: Round
Optional Features | Connection: Oval / Victaulic VFD on motor Single & Three phase motors High Efficiency motors Flameproof motors
Material of Construction | Casing – SS (304/316L) / Cast Iron Impeller – SS (304/316L)
Applications | Water Supply Pressure Boosting Jockey pump firefighting Boiler feed, Industrial Washing Sprinkling Systems General Industry
Prime movers | Electric motors

### FAQs of Vertical Inline Pump

A Vertical Inline Pump is a compact multistage centrifugal pump designed for pressure boosting, water transfer, and industrial applications where space-saving installation is important.

The pump can handle flow rates up to 155 m³/hr.

The pump delivers a head up to 235 meters.

The pump is suitable for liquid temperatures up to 120°C.

The pump is available in sizes ranging from DN 25 to DN 100.

Enquiry Now