- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Forged Steel – Gate, Globe & Lift Check Valves

### Model No: IVGTF / IVGLF / IVLCHF

Model: | IVGTF / IVGLF / IVLCHF
Size Range: | 15NB to 50NB
Pressure Rating: | ASME Class #150 to Class #2500
Design Standard: | API 602
Testing Std: | API 598
Face to Face: | Manufacturing Standard
End Connection: | Flanged, Socket Weld, Screwed & Butt Weld
Trim Options: | 1 / 5 / 8 / 12/ 16

### FAQs of Forged Steel – Gate, Globe & Lift Check Valves

These are compact and high-strength forged steel valves designed for isolation, flow regulation, and non-return applications in high pressure and high temperature piping systems.

- Gate Valve – Used for on-off isolation service
- Globe Valve – Used for flow control and throttling
- Lift Check Valve – Prevents reverse flow automatically

The valves are available in sizes ranging from 15 NB to 50 NB.

Yes. Forged steel construction and suitable trim selections make these valves ideal for severe service applications involving high pressure and temperature.

The valves are manufactured according to:

- Manufacturing Standard

Enquiry Now