- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Floating Ball Valve 2 Pcs Design Soft Seated

### Model No: R-Series

Model: | R-Series
Size Range: | 15 NB to 250 NB
Pressure Rating: | ASME Class #150, #300, #600
Design Standard: | ISO 17292, API 608, API 6D
Testing Std: | API 6D / BS EN ISO 5208 / API 598 / BS EN 12266-1
Face to Face: | ASME B 16.10
End Connection: | Flanged
Seat Design: | PTFE / MPTFE / TFM 1600 / RPTFE / DEVLON / PEEK

### FAQs of Floating Ball Valve 2 Pcs Design Soft Seated

A Floating Ball Valve is a quarter-turn shut-off valve in which the ball is free-floating and held between resilient seats. Line pressure pushes the ball against the downstream seat, ensuring tight sealing and reliable shutoff.

The valve is available in sizes ranging from 15 NB to 250 NB.

Floating Ball Valves are primarily designed for on-off isolation service. Limited throttling may be possible, but continuous throttling is generally not recommended.

The valve complies with:

- ASME B16.10
Enquiry Now