- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Mechanical Vacuum Boosters

100% Dry Pumping (No Sealing Fluid)
Current Range varies from 400 m3/hr to 30,000 m3/hr
High volumetric efficiency with great reliability
Internals available as per process requirements and applications

### FAQs of Mechanical Vacuum Boosters

A Mechanical Vacuum Booster is a positive displacement vacuum pump designed to increase pumping speed and improve the performance of primary vacuum systems in industrial applications.

Mechanical Vacuum Boosters are available in capacities ranging from 400 m³/hr to 30,000 m³/hr.

Dry pumping means the vacuum process occurs without any sealing fluids or lubricants in the pumping chamber, eliminating contamination risks and reducing maintenance requirements.

These boosters are engineered for exceptional durability, offering high reliability even in continuous and demanding operating environments.

Enquiry Now