- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### End Suction - Monobloc Pump

Flow up to | 110 m3/hr
Head up to | 80 m
Temperature up to | 60°C
DN | 40-80
Design Features | Mounting: Horizontal Monobioc design Stage: Single With TEFC enclosures & class F, Insulated IP44 motors (2 – 30 hp*) Mechanical Seal/ Gland Packing Pregreased, double sealed bearings
Optional Features | Submersible Monobloc design Single & Three phase motors IP 55 motors
Material of Construction | Casing – Cast Iron Impeller – Cast Iron / Bronze
Applications | Irrigation Water Supply HVAC Fire fighting General Industry
Prime movers | Electric motors

### FAQs of End Suction - Monobloc Pump

An End Suction Monobloc Pump is a compact centrifugal pump where the pump and motor are directly coupled into a single unit, providing efficient and space-saving operation.

The pump can handle flow rates up to 110 m³/hr.

The pump delivers a head up to 80 meters.

The pump is suitable for liquid temperatures up to 60°C.

The pump is available in sizes ranging from DN 40 to DN 80.

Enquiry Now