- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Engineered Horizontal Split Case Pump

Flow up to | 18000 m3/hr
Head up to | 270 m
Temperature up to | 120°C
DN | 50-1200
Design Features | Mounting Inline Horizontal Stage: One/ Two/Three stage single/ Double suction Impellers Grease/ Oil lubricated antifriction bearings Mechanical seal/ Gland Packing
Optional Features | Mounting: Centre line/vertical Drive Connection: Direct/Cardan Shaft Bush Bearing Staggered vane design for Fan Pump application Special Suction/ Delivery orientation Instrumentation & Controls
Material of Construction | Cast Iron, Bronze, Ductile Iron, Cast Steel, Ni Resist, stainless Steel, Duplex Stainless Steel & Special alloys
Applications | Water Supply General Industry Ports & Docks Firefighting Irrigation Marine Desalination
Prime movers | Electric motors/ Diesel Engines Steam Turbine with gear box or cardan shaft

### FAQs of Standard Horizontal Split Case Pump

An Engineered Horizontal Split Case Pump is a heavy-duty, high-capacity centrifugal pump designed for demanding industrial and infrastructure applications requiring high flow and pressure performance.

The pump can deliver flow rates up to 18,000 m³/hr.

The pump delivers a head up to 270 meters.

The pump is suitable for liquid temperatures up to 120°C.

The pump is available in sizes ranging from DN 50 to DN 1200.

Enquiry Now