- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Replacable Seats Butterfly Valve

### Model No: IVGK/IVTL

Model: | IVGK/IVTL
Size Range: | 50 NB to 600 NB
Pressure Rating: | Upto PN10
Design Standard: | API 609 , EN593, IS 13095
Testing Std: | API 598 / ANSI-FCI 70-2 / EN 12266-1
Face to Face: | API 609 Cat-A /ISO 5752 Tab 5/ BS EN558
End Connection: | Wafer / Lugged
Seat Design: | Replaceable

### FAQs of Replacable Seats Butterfly Valve

We offer a complete range including concentric, eccentric, and triple-offset butterfly valves, engineered for precise flow control, low torque operation, and long-term reliability across various industrial applications.

These models are available in sizes ranging from 50 NB to 600 NB, meeting the requirements of small to large piping systems.

Yes. The IVGK / IVTL models feature a replaceable seat design, allowing easy maintenance and ensuring a longer service life, especially in corrosive or abrasive applications.

Absolutely. With erosion-resistant sealing surfaces and optimized low-friction operation, these valves are ideal for corrosive, hygienic, and general industrial environments.

Enquiry Now