- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Metal Seated Double Offset Butterfly Valve

### Model No: IVEX-M

Model: | IVEX-M
Size Range: | 50 NB to 600 NB
Pressure Rating: | ASME Class #150, #300
Design Standard: | API 609 , EN593
Testing Std: | API 598 / ANSI-FCI 70-2 –Class IV
Face to Face: | API 609 Cat-B
End Connection: | Wafer / Lugged / Double Flanged
Seat Design: | SS / Inconel

### FAQs of Metal Seated Double Offset Butterfly Valve

A Metal Seated Double Offset Butterfly Valve is a high-performance butterfly valve designed for high temperature, high pressure, and demanding industrial services. It uses a double offset disc arrangement with metal seating for enhanced durability and reliable shutoff.

The valve is available in sizes ranging from 50 NB to 600 NB.

Yes. The valve is suitable for both isolation and throttling applications in demanding industrial systems.

The valves are tested according to:

- API 598
- ANSI FCI 70-2 – Class IV

Enquiry Now