- ISO 9001:2015 | CMFRI CERTIFIED
- +91 98240 67931
- sales@industrial-enterprises.com

### Mechanical Vapour Recompressors

Available for flow rate from 50 kg/h to 6000 kg/h in a single machine
More than 200 running installations
Proven and Rugged design

### FAQs of Mechanical Vapour Recompressors

A Mechanical Vapour Recompressor is an energy-efficient system that compresses and recycles low-pressure vapor, allowing it to be reused as a heating medium in evaporation and distillation processes.

Our MVR systems are available for vapor flow rates ranging from 50 kg/h to 6,000 kg/h in a single machine.

The system captures low-pressure vapor, compresses it mechanically, and reuses the compressed vapor as a heat source, greatly reducing the need for fresh steam.

With over 200 successful installations, our MVR systems have demonstrated outstanding reliability across various industrial applications.

Enquiry Now